[Contents] [Prev] [Next] [Index] [Report an Error]

# map-class frame-relay

#### Syntax

[ no ] map-class frame-relay mapName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates a map class. Command is used when configuring Frame Relay end-to-end fragmentation and reassembly. The no version removes the map-class.

#### Options

- mapName—Name of the map class; use up to 64 characters

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]