[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring BGP-Related Settings for VPLS

You can use the show ip bgp commands listed in Table 93 to display BGP-related settings for VPLS instances in the L2VPN address family or in the VPLS address family.

Table 93: Commands for Monitoring VPLS BGP Settings

show ip bgp | show ip bgp neighbors paths
show ip bgp advertised-routes | show ip bgp neighbors received-routes
show ip bgp community | show ip bgp neighbors routes
show ip bgp community-list | show ip bgp network
show ip bgp dampened-paths | show ip bgp next-hops
show ip bgp filter-list | show ip bgp paths
show ip bgp flap-statistics | show ip bgp peer-group
show ip bgp l2vpn | show ip bgp quote-regexp
show ip bgp l2vpn vpls | show ip bgp regexp
show ip bgp neighbors | show ip bgp summary
show ip bgp neighbors dampened-routes | –

#### Related Topics

- Monitoring Layer 2 NLRI for VPLS Instances
- Monitoring BGP Next Hops for VPLS
- For more information about using these commands, see Configuring BGP Routing and Configuring BGP-MPLS Applications.

[Contents] [Prev] [Next] [Index] [Report an Error]