[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 neighbor

#### Syntax

ipv6 neighbor [ vrf vrfName ] ipv6Address interfaceType interfaceSpecifier hardwareAddress

no ipv6 neighbor [ vrf vrfName ] ipv6Address interfaceType interfaceSpecifier

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
vrf keyword and vrfName variable added in JUNOSe Release 7.2.0.

#### Description

Specifies a static entry in the IPv6 Neighbor Discovery cache. The no version removes the static entry from the IPv6 Neighbor Discovery cache.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- ipv6Address—IPv6 address that corresponds to the local data-link address
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- hardwareAddress—Local, 48-bit data-link address

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]