> - Download PDFs
> - peak-burst
> - Related Topics
> - Creating a Two-Rate Rate-Limit Profile

> # peak-burst

> #### Syntax

> peak-burst size { millisecond milliseconds }

> no peak-burst

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> milliseconds variable added in JUNOSe Release 8.1.0.

> #### Description

> Sets the peak burst for a rate-limit profile. The no version restores the default value, 100 ms; if 100ms is less than 8K, then 8K (8192).

> #### Options

> - size—Size in bytes in the range 1–4294967295
> - milliseconds—Milliseconds in the range 1–10000

> #### Mode

> Rate Limit Profile Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.