> - Download PDFs
> - source-address

> # source-address

> #### Syntax

> source-address sourceAddress

> no source-address

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Specifies a source IP address for the LAC tunnel endpoint. The no version removes the source address.

> #### Options

> - sourceAddress—Address of the local tunnel endpoint (the LAC); can be up to 32 characters (no spaces)

> #### Mode

> Domain Map Tunnel Configuration, Tunnel Group Tunnel Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.