[Contents] [Prev] [Next] [Index] [Report an Error]

# redistribute isis

#### Syntax

[ no] redistribute isis from { level-1 into level-2 | level-2 into level-1 }
route-map mapTag

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Redistributes IPv6 routes from one IS-IS routing level into the other. The no version ends the redistribution.

#### Options

- level-1—Specifies the redistribution of routes from or into IS-IS level 1
- level-2—Specifies the redistribution of routes from or into IS-IS level 2
- mapTag—String of up to 32 alphanumeric characters specifying the route map applied to all routes from the source protocol; if you do not specify a route map, all routes are redistributed

#### Mode

Address Family Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]