[Contents] [Prev] [Next] [Index] [Report an Error]

# show ipv6 tunnel-route

#### Syntax

show ipv6 tunnel-route [ vrf vrfName ] [ ipv6Address [ detail ] | ipv6Prefix [ detail ] ]
[ all ] [ protocol ] [ filter ]

#### Release Information

Command introduced in JUNOSe Release 7.1.0.
vrf keyword and vrfName variable added in JUNOSe Release 7.2.0.

#### Description

Displays current state of the IPv6 tunnel routing table.

#### Options

- vrfName—Name of the VRF
- ipv6Address—IPv6 address
- ipv6Prefix—Prefix of prefix list entry; in the format IPv6baseaddress / length; for example, 1::1/32
- detail—Displays detailed information about the specific route
- all—Displays all routes in the IPv6 tunnel routing table inserted from all protocols, not just the best routes
- protocol—The following protocols for which you want to display the best route or all routes in the tunnel routing table; no routes are displayed if routes for the specified protocol are not present in the tunnel routing table

  | Note: Other protocol options are available in the CLI, but they are not applicable to the tunnel routing table.

  - bgp-tunnel—Displays the BGP tunnel routes in the tunnel routing table
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]