[Contents] [Prev] [Next] [Index] [Report an Error]

# exception dump

#### Syntax

exception dump { except-srp | srp-only } { local | ipAddress [ directoryName ] }

no exception dump

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the location from and to which the router should transfer a core dump file. Core dumps are enabled and stored in local NVS by default. The no version disables the command.

#### Options

- except-srp—Generates core dump for all non-SRP modules
- srp-only—Generates core dump for only the SRP modules
- local—Nonvolatile storage memory
- ipAddress—IP address of the server to which the router will transfer the core dump file
- directoryName—Name of the directory on the server to which the router will transfer the core dump file

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]