[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Configuration, Statistics, and Status for VPLS Ports

Purpose

Display configuration, statistics, and status information for ports (interfaces) associated with a VPLS instance.

Action

To display information for VPLS ports:

    host1#show bridge vplsC port

        FastEthernet1/1.1
          Port Number: 1
          Operational Status: Up
          Admin Status: Up
          Snmp Link Status Trap: Disabled
          Max Learn: Unlimited
          Subscriber Policy: samplepolicy
          Statistics:
             In Octets:    2018
             In Frames:    15
             In Discards:  0
             In Errors:    0
             Out Octets:   1930
             Out Frames:   14
             Out Discards: 0
             Out Errors:   0
          Time since counters last reset: 00:10:55

          queue 0: traffic class best-effort, bound to bridge FastEthernet1/1.1
            Queue length 0 bytes
            Forwarded packets 14, bytes 2042
            Dropped committed packets 0, bytes 0
            Dropped conformed packets 0, bytes 0
            Dropped exceeded packets 0, bytes 0

        vpls vplsC
          Port Number: 2
          Operational Status: Up
          Admin Status: Up
          Snmp Link Status Trap: Disabled
          Max Learn: Unlimited
          Subscriber Policy: default Trunk
          Statistics:
             In Octets:    0
             In Frames:    0
             In Discards:  0
             In Errors:    0
             Out Octets:   0
             Out Frames:   0
             Out Discards: 0
             Out Errors:   0
          Time since counters last reset: 00:07:07

To display a summary of all ports configured for the specified VPLS instance:

    host1#show bridge vplsTest port brief
     Port            Interface              Status
    ------   -------------------------   ------------
    1        FastEthernet1/1.1           Up
    2        ATM10/1.1.1                 Up
    3        vpls vplsTest               Up

Meaning

Table 89 lists the show bridge port command output fields.

Table 89: show bridge port Output Fields

Field Name | Field Description
--- | ---
BridgeGroup | Name of the VPLS instance to which the interface belongs
Port Number | Port number on which this interface resides
Operational Status | Operational status of the physical interface: Up, Down, LowerLayerDown, NotPresent
Admin Status | State of the physical interface: Up, Down
Snmp Link Status Trap | Whether SNMP link status processing is enabled or disabled for the specified interface
Max Learn | Maximum number of dynamic MAC addresses that the interface can learn
Subscriber Policy | Name of the subscriber policy currently in effect for the interface
Statistics | Displays statistics information for the specified port
In Octets | Number of octets received on this interface
In Frames | Number of frames received on this interface
In Discards | Number of incoming packets discarded on this interface
In Errors | Number of incoming errors received on this interface
Out Octets | Number of octets transmitted on this interface
Out Frames | Number of frames transmitted on this interface
Out Discards | Number of outgoing packets discarded on this interface
Out Errors | Number of outgoing errors on this interface
Time since counters last reset | Elapsed time since statistics counters were last reset
queue | Hardware packet queue associated with the specified traffic class and interface
Queue length | Length of the queue, in bytes
Forwarded packets, bytes | Number of packets and bytes forwarded on this queue
Dropped committed packets, bytes | Number of committed packets and bytes that were dropped
Dropped conformed packets, bytes | Number of conformed packets and bytes that were dropped
Dropped exceeded packets, bytes | Number of exceeded packets and bytes that were dropped
vpls vplsName | Identifies the VPLS virtual core interface for the VPLS instance

Table 90 lists the show bridge port brief command output fields.

Table 90: show bridge port brief Output Fields

Field Name | Field Description
--- | ---
Port | Port number on which this interface resides
Interface | Interface type and specifier associated with the port
Status | Operational status of the physical interface: Up, Down, LowerLayerDown, NotPresent

#### Related Topics

- show bridge port

[Contents] [Prev] [Next] [Index] [Report an Error]