[Contents] [Prev] [Next] [Index] [Report an Error]

# ip rip

#### Syntax

[ no ] ip rip

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures RIP to run on the network specified by the network command. Uses the default values: send version is RIP version 1, receive version is RIP version 1 and version 2, authentication is not enabled. The no version deletes the RIP interface.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]