> - Download PDFs
> - snmp-server host
> - Related Topics
> - Monitoring SNMP Secure Packet Mirroring Traps

> # snmp-server host

> #### Syntax

> To specify the SNMP version, community, UDP port, trap category and trap severity:

> snmp-server host ipAddress [ version ver ] securityString [ udp-port port ]
> [ trapCategory ]* [ trapFilters trapFilter ]

> no snmp-server host ipAddress

> To specify the ping timeout and trap queue:

> snmp-server host ipAddress pingTimeOut timeOutValue
> [ trapQueue { drainRate queueDrainRate | full queueFull |
> size queueSize }
> [ drainRate queueDrainRate | full queueFull | size queueSize ]*]

> snmp-server host ipAddress trapQueue
> { drainRate queueDrainRate | full queueFull | size queueSize }
> [ drainRate queueDrainRate | full queueFull | size queueSize ]*
> [ pingTimeOut timeOutValue ]

> no snmp-server host ipAddress { pingTimeOut | trapQueue { drainRate | full | size } }

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> ip keyword added in JUNOSe Release 7.1.0.
> packetMirror keyword added in JUNOSe Release 7.2.0.

> #### Description

> Configures one or more hosts to receive an SNMP trap. The no version removes the specified host from the list of recipients.

> #### Options

> - ipAddress—IP address of the SNMP trap recipient
> - ver—SNMP protocol version for traps sent to host; one of the following values: v1, v2c, or v3
> - securityString—SNMP community string
> - port—UDP port number of SNMP trap recipient
> - trapCategory—SNMP trap category
>   - addrPool—Local address pool traps
>   - atmPing—E-series router proprietary ATM ping traps
>   - bfdmib—BFD MIB traps
>   - bgp—BGP state change traps
>   - bulkstats—Bulkstats file full and nearly full traps
>   - cliSecurityAlert—Security alerts traps
>   - dosProtectionPlatform—DoS protection platform traps
>   - dvmrp—DVMRP traps
>   - dvmrpUni—E-series router proprietary DVMRP traps
>   - environment—Power/temperature/fan traps
>   - fileXfer—File transfer status change traps
>   - inventory—Router inventory/status traps
>   - ip—Internet Protocol traps
>   - ldp—LDP traps
>   - link—SNMP linkUp/linkDown traps
>   - log—System log capacity traps
>   - mobileIpv4—Mobile IPv4 traps
>   - mplste—Mplste traps
>   - mrouter—Mrouter traps
>   - packetMirror—Secure packet mirroring traps; visible only if packet mirroring is enabled
>   - ospf—OSPF traps
>   - ping—Ping operation traps (in disman remops MIB)
>   - radius—RADIUS traps
>   - snmp—SNMP coldstart, warmstart, link, authenticationFailure traps
>   - traceroute—Traceroute operation traps (in disman remops MIB)
> - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
> - trapFilter—Minimum severity level for filtering traps sent to this host
>   - alert—Severity level 1
>   - critical—Severity level 2
>   - debug—Severity level 7
>   - emergency—Severity level 0
>   - error—Severity level 3
>   - informational—Severity level 6
>   - notice—Severity level 5
>   - warning—Severity level 4
> - timeOutValue—Ping timeout in minutes, in the range 1–90; default value is 1
> - trapQueue—Configures the SNMP trap queue for traps sent to this host
> - queueDrainRate—Maximum number of traps per second to be sent to the host, in the range 0–2147483647; default value is 0
> - queueFull—Method used to drop traps when the trap queue is full
>   - dropFirstIn—Drops the oldest trap in the queue
>   - dropLastIn—Drops the most recent trap added to the queue
> - queueSize—Maximum number of traps to be kept in the trap queue, in the range 32–214748364; default value is 32

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.