[Contents] [Prev] [Next] [Index] [Report an Error]

# neighbor allow

#### Syntax

[ no ] neighbor peerGroupName allow accessListName
[ max-peers maxNumberDynamicPeers ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the peer group so that it accepts inbound connections from any remote address that matches the access list. The no version removes the configuration.

#### Options

- peerGroupName—Name of a BGP peer group
- accessListName—Name of an access list that specifies remote addresses from which BGP connections may be accepted
- maxNumberDynamicPeers—Maximum number of dynamic peers that a member of the peer group may accept

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]