[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa tunnel ignore

#### Syntax

aaa tunnel ignore { nas-port | nas-port-type } { enable | disable }

no aaa tunnel ignore { nas-port | nas-port-type }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies whether to use the tunnel peer's NAS-Port [5] and NAS-Port-Type [61] attributes. The no version negates the command or restores the default of enable.

#### Options

- nas-port—Configures the tunnel peer's supplied nas-port value
- nas-port-type—Configures the tunnel peer's supplied nas-port-type value
- enable—Implements the feature; this is the default setting
- disable—Disables the feature

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]