[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp group limit

#### Syntax

ip igmp group limit groupLimit

no ip igmp group limit

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Limits the number of IGMP groups that an interface can accept. The no version restores the default situation, in which there is no limit to the number of IGMP groups that the interface accepts.

#### Options

- groupLimit—Maximum number of IGMP groups that an interface can accept in the range 0–64,000

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]