> - Download PDFs
> - set dhcp relay proxy timeout

> # set dhcp relay proxy timeout

> #### Syntax

> set dhcp relay proxy timeout hours

> no set dhcp relay proxy timeout

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Sets the time that the DHCP relay proxy waits for a renewal message from the DHCP client after a reboot or switchover occurs. The no version restores the default value.

> #### Options

> - hours—Number of hours for the timeout, in the range 1–168 (1 hour to 7 days); default value is 72 hours

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.