[Contents] [Prev] [Next] [Index] [Report an Error]

# Creating Policy Lists for VLANs

The following example creates a VLAN policy list named routeForVlan. The classifier group lowLatencyLowDrop uses the default precedence of 100.

1. Create the policy list routeForVlan.
   `
   host1(config)#vlan policy-list routeForVlan
   host1(config-policy-list)#
   `
2. Create the classification group.
   `
   host1(config-policy-list)#classifier-group lowLatencyLowDrop
   host1(config-policy-list-classifier-group)#
   `
3. Create a rule that adds the lowLatencyLowDrop traffic class for all packets that fall into the lowLatencyLowDrop classification.
   `
   host1(config-policy-list-classifier-group)#traffic-class lowLatencyLowDrop
   `
4. Add a rule that sets the drop precedence for all packets that fall into the lowLatencyLowDrop classification to green.
   `
   host1(config-policy-list-classifier-group)#color green
   `
5. Add a rule that sets the user-priority bits for all packets that fall into the lowLatencyLowDrop classification to 7.
   `
   host1(config-policy-list-classifier-group)#mark-user-priority 7
   `
6. Exit to Policy List Configuration mode, then add traffic class rules for packets that conform to different CLACLs.
   `
   host1(config-policy-list-classifier-group)#exit
   host1(config-policy-list)#classifier-group lowLatency
   host1(config-policy-list-classifier-group)#traffic-class lowLatency
   host1(config-policy-list-classifier-group)#exit
   host1(config-policy-list)#classifier-group excellentEffort
   host1(config-policy-list-classifier-group)#traffic-class excellentEffort
   host1(config-policy-list-classifier-group)#exit
   host1(config-policy-list)#classifier-group bestEffort
   host1(config-policy-list-classifier-group)#traffic-class bestEffort
   `
7. Exit Policy List Configuration mode to save the configuration.
   `
   host1(config-policy-list-classifier-group)#exit
   host1(config-policy-list)#exit
   host1(config)#
   `
8. Display the policy list.

       host1#show policy-list routeForVlan

                                         Policy Table
                                         ------ -----
       VLAN Policy routeForVlan
          Administrative state: enable
          Reference count:      0
          Classifier control list: lowLatencyLowDrop, precedence 100
             traffic-class lowLatencyLowDrop
             color green
             mark-user-priority 7
          Classifier control list: lowLatency, precedence 100
             traffic-class lowLatency
          Classifier control list: excellentEffort, precedence 100
             traffic-class excellentEffort
          Classifier control list: bestEffort, precedence 100
             traffic-class bestEffort

#### Related Topics

- vlan policy-list

[Contents] [Prev] [Next] [Index] [Report an Error]