[Contents] [Prev] [Next] [Index] [Report an Error]

# set dhcp relay proxy timeout

#### Syntax

set dhcp relay proxy timeout hours

no set dhcp relay proxy timeout

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the time that the DHCP relay proxy waits for a renewal message from the DHCP client after a reboot or switchover occurs. The no version restores the default value.

#### Options

- hours—Number of hours for the timeout, in the range 1–168 (1 hour to 7 days); default value is 72 hours

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]