[Contents] [Prev] [Next] [Index] [Report an Error]

# show bridge port

#### Syntax

show bridge { bridgeGroupName | vplsName } port [ portNumber ] [ brief | delta ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
vplsName variable added in JUNOSe Release 7.1.0.

#### Description

Displays configuration, statistics, and status information for ports (interfaces) associated with a bridge group or VPLS instance.

#### Options

- bridgeGroupName—Name of a bridge group specified with the bridge command
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- portNumber—Port number for which you want to display information; if you omit the port number, the router displays information for all ports that belong to the bridge group or to the VPLS instance
- brief—Displays the port number, interface type, interface specifier, and operational status for each port that belongs to the bridge group or to the VPLS instance
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring Configuration, Statistics, and Status for VPLS Ports in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]