[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 nd active-solicitations

#### Syntax

[ no ] ipv6 nd active-solicitations

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that the router can actively solicit neighbors that become stale (inactive). The no version disables the ability to actively solicit neighbors that become stale.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]