[Contents] [Prev] [Next] [Index] [Report an Error]

# hello interval

#### Syntax

hello interval seconds

no hello interval

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Specifies the interval between link-hello packets sent by LDP. The no version restores the default interval, 5 seconds.

#### Options

- seconds—Number of seconds, in the range 1–65535

#### Mode

LDP Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]