[Contents] [Prev] [Next] [Index] [Report an Error]

# show controllers sonet remote

#### Syntax

show controllers sonet { interfaceSpecifier [ :controllerSpecifier ] remote [ all ] }
[ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays information about the statistics on the remote device when MDL is configured on a T3 over channelized SONET interface or FDL is configured on either a T1 channel on a T3 over channelized SONET interface or a T1 over SONET/SDH interface.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- controllerSpecifier—One of the following:
  - For a section or line, there is no controllerSpecifier
  - For a T3 over channelized SONET interface, specified in the format
    pathChannel ds3-channel-number [ ds1-channel-number ]
    [ subchannelNumber ]
  - For a T1 over SONET/SDH interface, specified in the format
    pathChannel [ /pathPayload ] [ /tributaryGroup ] [ /tributaryNumber ]
    [ /channelGroup ]
    - pathChannel—Number of the path
    - pathPayload—Number of the payload within the path. In SONET mode, pathPayload is always 1. In SDH mode, pathPayload is the number of the TUG-3 group.
    - tributaryGroup—Number of the tributary group within the path. In SONET mode, tributary group is the number of the VT group. In SDH mode, tributary group is the number of the TUG-2 group.
    - tributaryNumber—Number of the tributary within the group. In SONET mode, tributaryNumber is the number of the VT. In SDH mode, tributaryNumber is the number of the TUG-1 group or tributary unit.
    - channelGroup—Number of the channel group
    - ds3-channel-number—Number of the ds3 channel
    - ds1-channel-number—Number of the ds1 channel in the range 1–28
    - subchannelNumber—Number of the subchannel in the range 1–24
- all—Shows statistics for all time intervals, rather than statistics for selected time intervals
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]