[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Shadow Nodes on Different Traffic-Class Groups

This example shows how to configure shadow nodes on different traffic-class groups. After adding the voice queue in the auto-strict priority group named strict, the system stacks the IP voice queue above the Ethernet port, the voice group, and the phantom node.

`

host1(config-qos-profile)#ethernet node
host1(config-qos-profile)#ethernet shadow-node scheduler profile shadow
host1(config-qos-profile)#ethernet queue traffic-class best-effort scheduler-profile default
host1(config-qos-profile)#vlan node
host1(config-qos-profile)#ip node
host1(config-qos-profile)#ip queue traffic-class video scheduler-profile default
host1(config-qos-profile)#ethernet group voice-group scheduler-profile strict
host1(config-qos-profile)#ip queue traffic-class voice scheduler-profile default

`

[Contents] [Prev] [Next] [Index] [Report an Error]