[Contents] [Prev] [Next] [Index] [Report an Error]

# suspicious-control-flow-detection protocol backoff-time

#### Syntax

suspicious-control-flow-detection protocol protocolValue backoff-time backoffTimeValue

no suspicious-control-flow-detection protocol protocolValue backoff-time

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Sets the backoff expiration time when the flow is no longer considered suspicious for a specific protocol. The no version restores the default value of 300 seconds for a protocol.

#### Options

- protocolValue—Name of the protocol
- backoffTimeValue—Period of time in seconds; 0 or a number in the range 10–1000; a value of zero means that a suspicious flow does not change to the nonsuspicious state because of a timeout; if the low threshold value is zero and the backoff time is zero, the flow is only considered no longer suspicious if the rate (in packets per second) goes to zero

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]