[Contents] [Prev] [Next] [Index] [Report an Error]

# l2vpn site-range

#### Syntax

l2vpn l2VpnName site-range siteRange

no l2vpn l2VpnName site-range

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Configures the maximum number of customer sites that can participate in the specified VPWS L2VPN. In a VPWS L2VPN configuration, each customer site is represented by a customer edge (CE) device located at the edge of the customer's network. The no version restores the default site range, 1.

#### Options

- l2VpnName—Name of the VPWS instance
- siteRange—Maximum number of sites that can participate in the VPWS domain, in the range 1–65535; default value is 1

#### Mode

Global Configuration

#### Related Topics

- Configuring an L2VPN Instance in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]