[Contents] [Prev] [Next] [Index] [Report an Error]

# bgp advertise-best-external-to-internal

#### Syntax

[ no ] bgp advertise-best-external-to-internal

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Causes the BGP selection process to select two best routes to every destination. BGP advertises to external peers the best route selected from the complete set of routes known to that destination. BGP advertises to internal peers the best route from the set of routes received from external and confederation peers. The no version restores the default condition, wherein BGP selects only one best route for each destination from the complete set of routes; if the best route was received from an internal peer, BGP does not advertise any route to that destination to the internal peers.

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]