[Contents] [Prev] [Next] [Index] [Report an Error]

# ip profile

#### Syntax

ip profile profileName

no ip profile

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Specifies the IP profile that the IPSec layer passes on to the IP layer upon request for upper-layer instantiation. The no version removes the association with this profile.

#### Options

- profileName—Name of the profile that you want the IPSec layer to pass to the IP layer upon request for upper-layer instantiation

#### Mode

IPSec Tunnel Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]