[Contents] [Prev] [Next] [Index] [Report an Error]

# show frame-relay interface

#### Syntax

show frame-relay interface [ interfaceType interfaceSpecifier ] [ members ]
[ brief ] [ delta ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays Frame Relay statistics for interfaces.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers :
  - serial
  - pos
  - mlframe-relay
  - tunnel—GRE tunnel
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- members—Displays the status of MLFR links
  - displays the status of all MLFR links if you specify the interface type mlframe-relay without a specifier for an MLFR bundle
  - displays the status of MLFR links in an MLFR bundle if you specify that bundle
- brief—Displays a summary of interface information
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]