[Contents] [Prev] [Next] [Index] [Report an Error]

# service ctrl-x-reboot

#### Syntax

[ no ] service ctrl-x-reboot

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables the Ctrl+x key combination to reboot the router at all times, except that the key combination has no effect if you are accessing the router through a Telnet session. The no version restores the default condition, disabled.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]