[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp oif-map

#### Syntax

[ no ] ip igmp oif-map mapName { interfaceType interfaceSpecifier | self }
[ groupPrefix [ sourcePrefix ] ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates an outgoing interface (OIF) map. The no version removes an outgoing interface map attribute or the entire outgoing interface map.

#### Options

- mapName—Name of the OIF map
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- self—Specifies that the multicast outgoing interface is the same as IGMP join interface
- groupPrefix—Group prefix in the form ipAddress/maskLength
- sourcePrefix—Source prefix in the form ipAddress/maskLength

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]