[Contents] [Prev] [Next] [Index] [Report an Error]

# hdlc down-when-looped

#### Syntax

[ no ] hdlc down-when-looped

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables loopback detection on a Cisco HDLC interface. Loopback detection is disabled by default. The no version disables loopback detection.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]