[Contents] [Prev] [Next] [Index] [Report an Error]

# set route-type

#### Syntax

set route-type { internal | internal-intra | internal-inter | external }

no set route-type

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets routes of the specified type. The no version removes the set clause from a route map.

#### Options

- internal—Internal route (including OSPF intra-area and interarea)
- internal-intra—Intra-area route
- internal-inter—Interarea route
- external—External route (BGP and OSPF type 1/2)

#### Mode

Route Map Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]