[Contents] [Prev] [Next] [Index] [Report an Error]

# show mpls l2transport interface

#### Syntax

show mpls l2transport interface
[ summary | [ interfaceType interfaceSpecifier ] [ brief | detail ] [ state not-up ] [ delta ] ]
[ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
summary keyword added in JUNOSe Release 8.0.0.

#### Description

Displays status and configuration information about layer 2 services over MPLS (also known as Martini, or layer 2 transport) on the router or on specific interfaces.

#### Options

- summary—Displays summary information about layer 2 services over MPLS
- interfaceType—Displays information only for the specified MPLS interface; if not specified, information for all interfaces is displayed
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- brief—Displays limited interface information
- detail—Provides expanded information about layer 2 services, rather than a summary
- state not-up—Displays information only about interfaces that are not up
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- See Monitoring MPLS Layer 2 Interfaces for Layer 2 Services over MPLS in JUNOSe BGP and MPLS Configuration Guide
- Monitoring the Policy Configuration of Layer 2 Services over MPLS

[Contents] [Prev] [Next] [Index] [Report an Error]