[Contents] [Prev] [Next] [Index] [Report an Error]

# router mld

#### Syntax

[ no ] router mld

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates and enables MLD on a virtual router; accesses MLD router configuration mode. The no version disables MLD on a virtual router.

| Note: This command is identical to the ipv6 router mld command.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]