[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 pim sparse-mode graceful-restart-duration

#### Syntax

ipv6 pim sparse-mode graceful-restart-duration seconds

no ipv6 pim sparse-mode graceful-restart-duration

#### Release Information

Command introduced in JUNOSe Release 10.0.0.

#### Description

Sets duration time for PIM sparse-mode graceful restart. The no version resets the duration to the default.

#### Options

- seconds—Restart duration in seconds; default value is 30 seconds

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]