[Contents] [Prev] [Next] [Index] [Report an Error]

# queue

#### Syntax

[ no ] { typeOfInterface | set | superset } queue traffic-class trafficClassName
[ queue-profile queueProfileName [ scheduler-profile schedProfileName ] |
scheduler-profile schedProfileName [ queue-profile queueProfileName ] ]
[ drop-profile dropProfileName ] [ statistics-profile statisticsProfileName ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
svlan keyword added in JUNOSe Release 7.1.0.

set and superset keywords added in JUNOSe Release 9.2.0.

#### Description

Specifies that a queue traffic class be configured for the selected interface type. The no version removes this rule from the QoS profile.

#### Options

- typeOfInterface—Interface type for queue traffic classes to be configured; atm, atm-vp, atm-vc, bridge, ethernet, fr-vc, ip, ipv6, ip-tunnel, l2tp-session, l2tp-tunnel, lsp, serial, server-port, svlan, vlan
- set—Configures a queue for an interface set
- superset—Configures a queue for an interface superset
- trafficClassName—Name of the traffic class
- queueProfileName—Name of the queue profile
- schedProfileName—Name of the scheduler profile
- dropProfileName—Name of the drop profile
- statisticsProfileName—Name of the statistics profile

#### Mode

QoS Profile Configuration

#### Related Topics

- Configuring a QoS Profile
- Configuring Shadow Nodes
- Configuring a Basic Parameter Definition for QoS Administrators
- Configuring Rate Statistics
- Configuring Event Statistics
- Attaching a QoS Profile to an Interface Superset or an Interface Set

[Contents] [Prev] [Next] [Index] [Report an Error]