[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp rx-connect-speed-when-equal

#### Syntax

[ no ] l2tp rx-connect-speed-when-equal

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Generates the L2TP receive (RX) speed AVP when the RX and TX speeds are equal. The no version disables generation of the RX speed AVP when the RX and TX speeds are equal.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]