[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring LDP Graceful Restart

Purpose

Display information about LDP graceful restart.

Action

To display information about LDP graceful restart:

    host1#show ldp graceful-restart
    LDP Graceful Restart is enabled
    Helper Mode is enabled
    Reconnect Time: 220 sec
    Recovery Time: 240 sec
    Max Recovery Time: 260 sec
    Neighbor Liveness Timer: 280 sec
      Peer 80.0.1.1:0, State: operational, Restarter Mode: disabled, Helper Mode: enabled
      Peer 80.0.3.3:0, State: operational, Restarter Mode: disabled, Helper Mode: enabled

| Note: The mpls keyword is optional and is provided for compatibility with non–E-series implementations.

Meaning

Table 35 lists the show ldp graceful restart command output fields.

Table 35: show ldp graceful restart Output Fields

Field Name | Field Description
--- | ---
LDP Graceful Restart | State of graceful restart, enabled or disabled
Helper Mode | State of graceful restart helper mode, enabled or disabled
Reconnect Time | Locally configured value for reconnect time, in seconds
Recovery Time | Locally configured value for recovery time, in seconds
Max Recovery Time | Locally configured value for max-recovery timer, in seconds
Neighbor Liveness Timer | Locally configured value for neighbor-liveness timer, in seconds
Peer | Address, state, and LDP graceful restart state for neighbor

#### Related Topics

- show ldp graceful-restart

[Contents] [Prev] [Next] [Index] [Report an Error]