[Contents] [Prev] [Next] [Index] [Report an Error]

# ppp fragmentation

#### Syntax

ppp fragmentation [ fragmentSize ]

no ppp fragmentation

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables fragmentation on an MLPPP link interface and optionally specifies the maximum fragment size, in octets, to be used on the link. The no version disables fragmentation on the link and restores the default fragment size, which is the link’s MTU.

#### Options

- fragmentSize—Maximum allowable size of the fragment, in the range 128–65535; the default fragment size is the link’s MTU

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]