[Contents] [Prev] [Next] [Index] [Report an Error]

# shaping-rate

#### Syntax

shaping-rate shapingRate [ operator operandValue ]* [ bps | kbps ]
[ burst burstSize [ milliseconds | bytes ] ]

shaping-rate operandValue [ operator operandValue ]* [ bps | kbps ]

`

no shaping-rate

`

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
milliseconds and bytes keywords added in JUNOSe Release 7.1.0.
bps and kbps keywords added in JUNOSe Release 8.0.0.

#### Description

Sets the shaping rate and burst size. The no version deletes the shaping rate.

#### Options

- shapingRate—Constant shaping rate in bits per second; in the range 1000–1000000000 (1 Kbps–1000 Kbps)
- operator—Mathematical function
- operandValue—Input for the operator; can be a QoS parameter definition name or an integer
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- bps—Specifies shaping rate in bits per second
- kbps—Specifies shaping rate in kilobits per second
- burstSize—Number, in the range 0–522240 (0–510 KB); 0 enables the router to select an applicable default value
- milliseconds—Specifies burst size in milliseconds
- bytes—Specifies burst size in bytes

#### Mode

Scheduler Profile Configuration

#### Related Topics

- Configuring Rate Shaping for a Scheduler Node or Queue
- Configuring Port Shaping
- Configuring a Basic Parameter Definition for QoS Administrators

[Contents] [Prev] [Next] [Index] [Report an Error]