[Contents] [Prev] [Next] [Index] [Report an Error]

# undebug ip bgp

#### Syntax

undebug ip bgp [ in | out ] [ peerAddress [ peerAddressMask ] ]
[ bgpLog ] [ router routerName ] [ filtering-router filteringRouterName ]
[ accessClassName ] [ route-map mapName ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Turns off the display of information previously enabled with the debug ip bgp command. There is no no version.

#### Options

- in—Displays information for inbound events
- out—Displays information for outbound events
- peerAddress—IP address of BGP peer for which information is displayed
- peerAddressMask—Network mask of BGP peer for which information is displayed
- bgpLog—BGP log of interest; one of the following options:
  - dampening—BGP dampening event; route is suppressed or no longer suppressed by route-flap dampening
  - events—BGP finite state machine events and transitions
  - keepalives—BGP keepalive message events
  - next-hops—BGP next hop events
  - updates—BGP routing table update events
- routerName—Name of the virtual router that owns the BGP router for which information is being displayed
- filteringRouterName—Name of the virtual router that owns the access class and route map parameters
- accessClassName—Name of an access list to filter output
- mapName—Name of a route map to filter output

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]