[Contents] [Prev] [Next] [Index] [Report an Error]

# set dhcp relay assign-giaddr-source-ip

#### Syntax

[ no ] set dhcp relay assign-giaddr-source-ip

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Configures DHCP relay and DHCP relay proxy to assign the gateway IP address (giaddr) to the source IP address of traffic they send to DHCP servers. The no version restores the default, in which the DHCP relay and DHCP relay proxy do not assign the giaddr to the source IP address.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]