[Contents] [Prev] [Next] [Index] [Report an Error]

# atm vp-description

#### Syntax

atm vp-description vpi description

no atm vp-description vpi

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Assigns a text description to an individual virtual path (VP) on an ATM interface. Use the show atm vp-description command to display the description. The no version restores the default value, a null string.

#### Options

- vpi—Virtual path identifier number in the range 0–255
- description—Text string or alias for the specified VPI; up to 32 characters

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]