[Contents] [Prev] [Next] [Index] [Report an Error]

# ip router-id

#### Syntax

[ no ] ip router-id [ vrfName ] ipAddress

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Establishes the IP address of a router. The no version removes the IP address assignment.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- ipAddress—IP address of the router

#### Mode

Global Configuration

#### Related Topics

- Configuring the Loopback Interface and Router ID for BGP for L2VPNs and Configuring the Loopback Interface and Router ID for VPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]