[Contents] [Prev] [Next] [Index] [Report an Error]

## atm

#### Description

ATM interface

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Unable to reenable ILMI administrative state after UNI version change

#### Warning Log

Error getting location of underlying physical interface; error binding or unbinding to physical interface; error allocating memory for new interface; error setting system identifier; error adding or configuring an interface; error getting capabilities of interface; error getting maximum VPI/VCI for interface; error getting maximum virtual circuit descriptor for interface; unable to store or allocate memory for F4 OAM circuit data; unable to configure F4 OAM circuit for interface

#### Notice Log

Interface pool expanded by an incremental number of entries; report retry delay in seconds when waiting for the underlying physical interface to be created; unable to allocate a message to send an interface up or down notification; unable to add or configure interface

#### Info

Dropping interface up, down, or not present notification due to removal of interface; discarding F4 OAM circuits when interface does not support F4 OAM

#### Debug

None

#### Filter

None

[Contents] [Prev] [Next] [Index] [Report an Error]