[Contents] [Prev] [Next] [Index] [Report an Error]

# priority over-subscription-factor

#### Syntax

priority priorityValue over-subscription-factor oversubscriptionValue

no priority priorityValue over-subscription-factor

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Sets the oversubscription value for each priority rate limiter. The no version returns to the default value.

#### Options

- priorityValue—Hi-Green-IC, Hi-Green-SC, Hi-Yellow-IC, Hi-Yellow-SC, Lo-Green-IC, Lo-Green-SC, Lo-Yellow-IC, Lo-Yellow-SC
- oversubscriptionValue—Percentage of packets in the range 100–1000; default value is 500

#### Mode

DoS Protection Group Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]