[Contents] [Prev] [Next] [Index] [Report an Error]

# atm aal5 shutdown

#### Syntax

[ no ] atm aal5 shutdown

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the administrative state of an ATM AAL5 interface to disabled. The no version enables a disabled interface.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]