[Contents] [Prev] [Next] [Index] [Report an Error]

# profile atm1483 bulk-config-name

#### Syntax

profile atm1483 bulk-config-name bulkConfigName profileName

no profile atm1483 bulk-config-name bulkConfigName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Assigns the base profile configured for a dynamic ATM 1483 subinterface to the VC range configured on a static ATM AAL5 interface with the atm bulk-config command. The no version removes the profile assignment.

#### Options

- bulkConfigName—Name associated with the VC range on the static ATM AAL5 interface, as specified in the atm bulk-configcommand
- profileName—Base profile name associated with the dynamic ATM 1483 subinterface

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]