[Contents] [Prev] [Next] [Index] [Report an Error]

# show l2tp dial-out

#### Syntax

show l2tp dial-out [ [ detail ] [ state operState ] | summary ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays the chassis-wide configuration, operational state, and statistics for L2TP dial-out.

#### Options

- detail—Displays configuration, states, and statistics
- operState—One of the following operational states:
  - inService
  - initIncomplete
  - restricted
- summary—Displays aggregate counts for virtual routers, targets, and sessions in each of the possible operational and administrative states
- filter—See Filtering show Commands

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]