[Contents] [Prev] [Next] [Index] [Report an Error]

# peak-burst

#### Syntax

peak-burst size { millisecond milliseconds }

no peak-burst

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
milliseconds variable added in JUNOSe Release 8.1.0.

#### Description

Sets the peak burst for a rate-limit profile. The no version restores the default value, 100 ms; if 100ms is less than 8K, then 8K (8192).

#### Options

- size—Size in bytes in the range 1–4294967295
- milliseconds—Milliseconds in the range 1–10000

#### Mode

Rate Limit Profile Configuration

#### Related Topics

- Creating a Two-Rate Rate-Limit Profile

[Contents] [Prev] [Next] [Index] [Report an Error]