[Contents] [Prev] [Next] [Index] [Report an Error]

# mark-clp

#### Syntax

[ no ] [ suspend ] mark-clp clpValue

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Marks the CLP bit in the ATM header of packets matching the current classifier control list. The no version removes the mark rule from a policy list; the suspend version temporarily suspends a mark rule; the no suspend version resumes application of a suspended rule.

#### Options

- clpValue—Value of the CLP bit, 0 or 1

#### Mode

Classifier Group Configuration

#### Related Topics

- Assigning Values to the ATM CLP Bit
- Policy Rule Precedence

[Contents] [Prev] [Next] [Index] [Report an Error]